Package: 6in4
Version: 14-1
Depends: libc, kmod-ipv6, kmod-sit
Source: package/network/ipv6/6in4
Section: ipv6
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: all
Installed-Size: 1168
Filename: 6in4_14-1_all.ipk
Size: 1811
MD5Sum: dc7237174c049b6b8f5c21416b7486bb
Description:  Provides support for 6in4 tunnels in /etc/config/network.
 Refer to http://wiki.openwrt.org/doc/uci/network for
 configuration details.

Package: 6rd
Version: 3-1
Depends: libc, kmod-ipv6, kmod-sit
Source: package/network/ipv6/6rd
Section: ipv6
Maintainer: Stéphan Kochen <stephan@kochen.nl>
Architecture: all
Installed-Size: 2828
Filename: 6rd_3-1_all.ipk
Size: 3448
MD5Sum: 6719e5b5b28aa1f26a892eee56a0ce6d
Description:  Provides support for 6rd tunnels in /etc/config/network.
 Refer to http://wiki.openwrt.org/doc/uci/network for
 configuration details.

Package: 6relayd
Version: 2013-02-28.1-be18c9722e8fa76ca96de16fb927b85bfe3197bc
Depends: libc, kmod-ipv6
Source: package/network/ipv6/6relayd
SourceFile: 6relayd-2013-02-28.1.tar.bz2
SourceURL: git://github.com/sbyx/6relayd.git
Section: ipv6
Maintainer: Steven Barth <steven@midlink.org>
Architecture: ar71xx
Installed-Size: 13696
Filename: 6relayd_2013-02-28.1-be18c9722e8fa76ca96de16fb927b85bfe3197bc_ar71xx.ipk
Size: 14580
MD5Sum: e848d5850f653dd73498197496fdafa4
Description:  6relayd is an IPv6-tool that relays IPv6-management protocols like router
 discovery, neighbor discovery and DHCPv6 so that clients on routed (non-
 bridged) interfaces can use the public address prefix, DHCPv6 and DNS-service
 of a master interface. This is useful to avoid NAT in chained IPv6-routers.
 
 It can also be used as a lightweight router advertisement daemon and provide
 stateless DHCPv6 service where size matters.

Package: 6to4
Version: 12-1
Depends: libc, kmod-ipv6, kmod-sit
Source: package/network/ipv6/6to4
Section: ipv6
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: all
Installed-Size: 1008
Filename: 6to4_12-1_all.ipk
Size: 1638
MD5Sum: dd31c7cf4d72b606325ed81c680f3ec9
Description:  Provides support for 6to4 tunnels in /etc/config/network.
 Refer to http://wiki.openwrt.org/doc/uci/network for
 configuration details.

Package: base-files
Version: 134-r36006
Depends: libc, netifd, procd
Source: package/base-files
Section: base
Architecture: ar71xx
Installed-Size: 45808
Filename: base-files_134-r36006_ar71xx.ipk
Size: 46532
MD5Sum: 4165c0a9ad602eb0e541e10cd6a538cd
Description:  This package contains a base filesystem and system scripts for OpenWrt.

Package: busybox
Version: 1.19.4-6
Depends: libc
Source: package/busybox
SourceFile: busybox-1.19.4.tar.bz2
SourceURL: http://www.busybox.net/downloads http://distfiles.gentoo.org/distfiles/
License: GPLv2 BSD-4c
LicenseFiles: LICENSE archival/libarchive/bz/LICENSE
Section: base
Essential: yes
Maintainer: Nicolas Thill <nico@openwrt.org>
Architecture: ar71xx
Installed-Size: 236223
Filename: busybox_1.19.4-6_ar71xx.ipk
Size: 235030
MD5Sum: 35cfa69bd9b5e864f170ea1df9cf20bd
Description:  The Swiss Army Knife of embedded Linux.
 It slices, it dices, it makes Julian Fries.

Package: chat
Version: 2.4.5-9
Depends: libc
Source: package/network/services/ppp
SourceFile: ppp-2.4.5.tar.gz
SourceURL: ftp://ftp.samba.org/pub/ppp/
Section: net
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: ar71xx
Installed-Size: 8684
Filename: chat_2.4.5-9_ar71xx.ipk
Size: 9380
MD5Sum: eb3ea5dd04404ab70d7385f98dacef4c
Description:  This package contains an utility to establish conversation with other PPP servers
 (via a modem).

Package: comgt
Version: 0.32-21
Depends: libc, chat
Source: package/network/utils/comgt
SourceFile: comgt.0.32.tgz
SourceURL: @SF/comgt
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 19823
Filename: comgt_0.32-21_ar71xx.ipk
Size: 20457
MD5Sum: eee0860313baebab072f04379f8e6e10
Description:  comgt is a scripting language interpreter useful for establishing 
 communications on serial lines and through PCMCIA modems as well as GPRS 
 and 3G datacards.

Package: ddns-scripts
Version: 1.0.0-21
Depends: libc
Source: feeds/packages/net/ddns-scripts
Section: net
Architecture: all
Installed-Size: 6705
Filename: ddns-scripts_1.0.0-21_all.ipk
Size: 7334
MD5Sum: d9dc57fc3da563694e671705651f35d9
Description:  A highly configurable set of scripts for doing
 dynamic dns updates

Package: dnsmasq-dhcpv6
Version: 2.62-3
Depends: libc, kmod-ipv6
Source: package/network/services/dnsmasq
SourceFile: dnsmasq-2.62.tar.gz
SourceURL: http://thekelleys.org.uk/dnsmasq
License: GPLv2
LicenseFiles: COPYING
Section: net
Architecture: ar71xx
Installed-Size: 98193
Filename: dnsmasq-dhcpv6_2.62-3_ar71xx.ipk
Size: 98480
MD5Sum: 15d79aed541f8275f4310f28e1315467
Description:  It is intended to provide coupled DNS and DHCP service to a LAN.
 
 This is a variant with DHCPv6 support

Package: dnsmasq
Version: 2.62-3
Depends: libc
Source: package/network/services/dnsmasq
SourceFile: dnsmasq-2.62.tar.gz
SourceURL: http://thekelleys.org.uk/dnsmasq
License: GPLv2
LicenseFiles: COPYING
Section: net
Architecture: ar71xx
Installed-Size: 82513
Filename: dnsmasq_2.62-3_ar71xx.ipk
Size: 82826
MD5Sum: 25644044e71d0fcd0c23b9b3f3d6fefb
Description:  It is intended to provide coupled DNS and DHCP service to a LAN.

Package: dropbear
Version: 2012.55-2
Depends: libc
Source: package/network/services/dropbear
SourceFile: dropbear-2012.55.tar.bz2
SourceURL: http://matt.ucc.asn.au/dropbear/releases/ http://www.mirrors.wiretapped.net/security/cryptography/apps/ssh/dropbear/
License: MIT
LicenseFiles: LICENSE libtomcrypt/LICENSE libtommath/LICENSE
Section: net
Architecture: ar71xx
Installed-Size: 78528
Filename: dropbear_2012.55-2_ar71xx.ipk
Size: 78761
MD5Sum: d99db46c5611e6715501d61494a91e8d
Description:  A small SSH2 server/client designed for small memory environments.

Package: firewall3
Version: 2013-03-13
Depends: libc, libubox, libubus, libuci
Source: package/network/config/firewall3
SourceFile: firewall3-2013-03-13-ff9d5e13c9150c62fe698e4bc5541e6f92b241d0.tar.gz
SourceURL: git://nbd.name/firewall3.git
Section: net
Maintainer: Jo-Philipp Wich <jow@openwrt.org>
Architecture: ar71xx
Installed-Size: 25726
Filename: firewall3_2013-03-13_ar71xx.ipk
Size: 26378
MD5Sum: 6ffbce414d2d39e9463c4b81d561af71
Description:  This package provides a config-compatible C implementation of the UCI firewall.

Package: firewall
Version: 2-59
Depends: libc, iptables, kmod-ipt-conntrack, kmod-ipt-nat
Source: package/network/config/firewall
Section: net
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: all
Installed-Size: 13261
Filename: firewall_2-59_all.ipk
Size: 13877
MD5Sum: 9f797bb61a1ceecc74bef630226c6f02
Description:  UCI based firewall for OpenWrt

Package: hotplug2
Version: 1.0-beta-4
Depends: libc
Source: package/hotplug2
SourceFile: hotplug2-201.tar.gz
SourceURL: http://svn.nomi.cz/svn/isteve/hotplug2
Section: base
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 14483
Filename: hotplug2_1.0-beta-4_ar71xx.ipk
Size: 15030
MD5Sum: fdf19fc039c854f169bafe9ec9d7449e
Description:  Hotplug2 is a trivial replacement of some of the UDev functionality
 in a tiny pack, intended for Linux early userspace: Init RAM FS and InitRD.
 This is an implementation of Hotplug2-1.0-beta

Package: ip6tables
Version: 1.4.18-2
Depends: libc, kmod-ip6tables, iptables
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: net
Architecture: ar71xx
Installed-Size: 215
Filename: ip6tables_1.4.18-2_ar71xx.ipk
Size: 819
MD5Sum: 1b246a4b039ac9cddf39c2fcdfcbf7db
Description:  IPv6 firewall administration tool

Package: ip
Version: 3.7.0-1
Depends: libc, libnl-tiny
Source: package/network/utils/iproute2
SourceFile: iproute2-3.7.0.tar.bz2
SourceURL: http://kernel.org/pub/linux/utils/net/iproute2/
Section: net
Architecture: ar71xx
Installed-Size: 91889
Filename: ip_3.7.0-1_ar71xx.ipk
Size: 92338
MD5Sum: a39568bc563541e766cce6cfef92d0e9
Description:  Routing control utility

Package: iptables-mod-conntrack-extra
Version: 1.4.18-2
Depends: libc, iptables, kmod-ipt-conntrack-extra
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: net
Architecture: ar71xx
Installed-Size: 7612
Filename: iptables-mod-conntrack-extra_1.4.18-2_ar71xx.ipk
Size: 8296
MD5Sum: b6acf15de4d9b2c040479cf704df01e2
Description:  Extra iptables extensions for connection tracking.
 
 Matches:
 - connbytes
 - connmark
 - recent
 - helper
 
 Targets:
 - CONNMARK
 

Package: iptables-mod-filter
Version: 1.4.18-2
Depends: libc, iptables, kmod-ipt-filter
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: net
Architecture: ar71xx
Installed-Size: 14482
Filename: iptables-mod-filter_1.4.18-2_ar71xx.ipk
Size: 15121
MD5Sum: 669f6f55de415b48e82f0e7975a6951a
Description:  iptables extensions for packet content inspection.
 Includes support for:
 
 Matches:
 - layer7
 - string
 

Package: iptables-mod-ipopt
Version: 1.4.18-2
Depends: libc, iptables, kmod-ipt-ipopt
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: net
Architecture: ar71xx
Installed-Size: 18332
Filename: iptables-mod-ipopt_1.4.18-2_ar71xx.ipk
Size: 19012
MD5Sum: e003208c90f9b6bf15cf2851f13b6161
Description:  iptables extensions for matching/changing IP packet options.
 
 Matches:
 - dscp
 - ecn
 - length
 - mark
 - statistic
 - tcpmss
 - time
 - unclean
 - hl
 
 Targets:
 - DSCP
 - CLASSIFY
 - ECN
 - MARK
 - HL
 

Package: iptables
Version: 1.4.18-2
Depends: libc, kmod-ipt-core, libip4tc, libip6tc, libxtables
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: net
Architecture: ar71xx
Installed-Size: 45522
Filename: iptables_1.4.18-2_ar71xx.ipk
Size: 45792
MD5Sum: d9576b1474e3583fd55e6eaae06bd9de
Description:  IP firewall administration tool.
 
 Matches:
 - icmp
 - tcp
 - udp
 - comment
 - limit
 - mac
 - multiport
 
 Targets:
 - ACCEPT
 - DROP
 - REJECT
 - LOG
 - TCPMSS
 
 Tables:
 - filter
 - mangle
 

Package: ipv6-support
Version: 2013-01-23-1
Depends: libc, kmod-ipv6, 6relayd, odhcp6c, ip6tables
Source: package/network/ipv6/ipv6-support
Section: ipv6
Maintainer: Steven Barth <steven@midlink.org>
Architecture: all
Installed-Size: 375
Filename: ipv6-support_2013-01-23-1_all.ipk
Size: 1018
MD5Sum: 729af7d1a352cb9e1b50d27aec65ba9d
Description:  This package provides basic IPv6 support including Router Discovery,
 DHCPv6 (client & server), prefix delegation and distribution.

Package: iw
Version: 3.6-1
Depends: libc, libnl-tiny
Source: package/network/utils/iw
SourceFile: iw-3.6.tar.bz2
SourceURL: http://wireless.kernel.org/download/iw/
Section: net
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 36536
Filename: iw_3.6-1_ar71xx.ipk
Size: 37204
MD5Sum: 98b38b06b07fdab8f42b660c9b99b4ce
Description:  cfg80211 interface configuration utility

Package: jshn
Version: 2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442
Depends: libc, libjson
Source: package/libs/libubox
SourceFile: libubox-2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442.tar.gz
SourceURL: git://nbd.name/luci2/libubox.git
License: ISC BSD-3c
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 4991
Filename: jshn_2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442_ar71xx.ipk
Size: 5657
MD5Sum: 93db1c30bd9aa9cd387071844256aed6
Description:  Library for parsing and generating JSON from shell scripts

Package: kmod-ath9k-common
Version: 3.8.2+2013-02-22-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ath
Source: package/mac80211
SourceFile: compat-wireless-2013-02-22.tar.bz2
SourceURL: http://mirror2.openwrt.org/sources
Section: kernel
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 116526
Filename: kmod-ath9k-common_3.8.2+2013-02-22-1_ar71xx.ipk
Size: 114072
MD5Sum: 3826d87cf9819365b534150c77da4c44
Description:  Atheros 802.11n wireless devices (common code for ath9k and ath9k_htc)

Package: kmod-ath9k
Version: 3.8.2+2013-02-22-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ath9k-common
Source: package/mac80211
SourceFile: compat-wireless-2013-02-22.tar.bz2
SourceURL: http://mirror2.openwrt.org/sources
Section: kernel
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 55164
Filename: kmod-ath9k_3.8.2+2013-02-22-1_ar71xx.ipk
Size: 55589
MD5Sum: 83f1ad821d7f0f6a3ec3173c3bdd4263
Description:  This module adds support for wireless adapters based on
 Atheros IEEE 802.11n AR5008 and AR9001 family of chipsets.

Package: kmod-ath
Version: 3.8.2+2013-02-22-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-mac80211
Source: package/mac80211
SourceFile: compat-wireless-2013-02-22.tar.bz2
SourceURL: http://mirror2.openwrt.org/sources
Section: kernel
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 9450
Filename: kmod-ath_3.8.2+2013-02-22-1_ar71xx.ipk
Size: 9997
MD5Sum: e4cc84789f52c26135c87e825c75f4f7
Description:  This module contains some common parts needed by Atheros Wireless drivers.

Package: kmod-cfg80211
Version: 3.8.2+2013-02-22-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), iw
Source: package/mac80211
SourceFile: compat-wireless-2013-02-22.tar.bz2
SourceURL: http://mirror2.openwrt.org/sources
Section: kernel
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 95197
Filename: kmod-cfg80211_3.8.2+2013-02-22-1_ar71xx.ipk
Size: 95573
MD5Sum: 55988a820b4dfb36c04bbd75df13f94a
Description:  cfg80211 is the Linux wireless LAN (802.11) configuration API.

Package: kmod-crypto-aes
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-crypto-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 105
Filename: kmod-crypto-aes_3.8.2-1_ar71xx.ipk
Size: 672
MD5Sum: f6c74b9d34aaebbe66acc6ebc0fb94ba
Description:  AES cipher CryptoAPI module

Package: kmod-crypto-arc4
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-crypto-core, kmod-crypto-manager
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1325
Filename: kmod-crypto-arc4_3.8.2-1_ar71xx.ipk
Size: 2057
MD5Sum: 6703edd9e398bf0b0f9d17866d9df91f
Description:  ARC4 (RC4) cipher CryptoAPI module

Package: kmod-crypto-core
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 105
Filename: kmod-crypto-core_3.8.2-1_ar71xx.ipk
Size: 663
MD5Sum: 53a613d49620dce8800a1121d953cfd6
Description:  Core CryptoAPI modules

Package: kmod-crypto-manager
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-crypto-hash, kmod-crypto-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 9306
Filename: kmod-crypto-manager_3.8.2-1_ar71xx.ipk
Size: 10043
MD5Sum: f36191ff030f8cfec7c9f5b0d2ce6345
Description:  CryptoAPI algorithm manager

Package: kmod-gpio-button-hotplug
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/system/gpio-button-hotplug
Section: kernel
Architecture: ar71xx
Installed-Size: 3699
Filename: kmod-gpio-button-hotplug_3.8.2-1_ar71xx.ipk
Size: 4352
MD5Sum: 38308db5727e7379ff279b0251ac9638
Description:  Simple GPIO Button Hotplug driver

Package: kmod-ifb
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 2966
Filename: kmod-ifb_3.8.2-1_ar71xx.ipk
Size: 3634
MD5Sum: 2d397259b1f95d1215dddd638ea6e6c5
Description:  The Intermediate Functional Block

Package: kmod-ip6tables
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipv6
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 22674
Filename: kmod-ip6tables_3.8.2-1_ar71xx.ipk
Size: 23354
MD5Sum: 2038a7889a7ba3d2e0772d21894c7dcc
Description:  Netfilter IPv6 firewalling support

Package: kmod-ipt-conntrack-extra
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core, kmod-ipt-conntrack
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 8413
Filename: kmod-ipt-conntrack-extra_3.8.2-1_ar71xx.ipk
Size: 9216
MD5Sum: 01760c50208b4654bbc3d50991eda0fd
Description:  Netfilter (IPv4) extra kernel modules for connection tracking
 Includes:
 - connbytes
 - connmark/CONNMARK
 - conntrack
 - helper
 - recent

Package: kmod-ipt-conntrack
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 34820
Filename: kmod-ipt-conntrack_3.8.2-1_ar71xx.ipk
Size: 35590
MD5Sum: 34d3505cdcaa99710505e74172c12243
Description:  Netfilter (IPv4) kernel modules for connection tracking
 Includes:
 - conntrack
 - defrag
 - iptables_raw
 - NOTRACK
 - state

Package: kmod-ipt-core
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 28687
Filename: kmod-ipt-core_3.8.2-1_ar71xx.ipk
Size: 29406
MD5Sum: d1ac3e6102d12e2543e5caa810cf0505
Description:  Netfilter core kernel modules
 Includes:
 - comment
 - limit
 - LOG
 - mac
 - multiport
 - REJECT
 - TCPMSS

Package: kmod-ipt-filter
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core, kmod-lib-textsearch
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 8290
Filename: kmod-ipt-filter_3.8.2-1_ar71xx.ipk
Size: 9050
MD5Sum: 92a37d74d7c32db0c0e98b36c3a0cc14
Description:  Netfilter (IPv4) kernel modules for packet content inspection
 Includes:
 - layer7
 - string

Package: kmod-ipt-ipopt
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 8497
Filename: kmod-ipt-ipopt_3.8.2-1_ar71xx.ipk
Size: 9325
MD5Sum: ccbd74ae6ba876f081246d1e7c5699e3
Description:  Netfilter (IPv4) modules for matching/changing IP packet options
 Includes:
 - CLASSIFY
 - dscp/DSCP
 - ecn/ECN
 - hl/HL
 - length
 - mark/MARK
 - statistic
 - tcpmss
 - time
 - ttl/TTL
 - unclean

Package: kmod-ipt-nat
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core, kmod-ipt-conntrack
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 12667
Filename: kmod-ipt-nat_3.8.2-1_ar71xx.ipk
Size: 13426
MD5Sum: 9817e6f4648b9abd2c7b66149a7a6c6f
Description:  Netfilter (IPv4) kernel modules for basic NAT targets
 Includes:
 - MASQUERADE

Package: kmod-ipt-nathelper-extra
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core, kmod-ipt-nat, kmod-lib-textsearch
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 48737
Filename: kmod-ipt-nathelper-extra_3.8.2-1_ar71xx.ipk
Size: 49580
MD5Sum: 35ffd54defeb61a899f85f38e60aa679
Description:  Extra Netfilter (IPv4) Conntrack and NAT helpers
 Includes:
 - amanda
 - h323
 - mms
 - pptp
 - proto_gre
 - sip
 - snmp_basic
 - broadcast

Package: kmod-ipt-nathelper
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipt-core, kmod-ipt-nat
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 7687
Filename: kmod-ipt-nathelper_3.8.2-1_ar71xx.ipk
Size: 8462
MD5Sum: bd1cd459200ab348d49bdac57045c0ef
Description:  Default Netfilter (IPv4) Conntrack and NAT helpers
 Includes:
 - ftp
 - irc
 - tftp

Package: kmod-iptunnel4
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1852
Filename: kmod-iptunnel4_3.8.2-1_ar71xx.ipk
Size: 2559
MD5Sum: c935e9515587b8c2909b174324ac35b3
Description:  Kernel modules for IPv4 tunneling

Package: kmod-ipv6
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 145959
Filename: kmod-ipv6_3.8.2-1_ar71xx.ipk
Size: 145986
MD5Sum: 90eda11aa2d8d61f714ddcda21b4545a
Description:  Kernel modules for IPv6 support

Package: kmod-leds-gpio
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1930
Filename: kmod-leds-gpio_3.8.2-1_ar71xx.ipk
Size: 2638
MD5Sum: e77b9c69d9229e9702754a8aa550a81b
Description:  Kernel module for LEDs on GPIO lines

Package: kmod-ledtrig-default-on
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 873
Filename: kmod-ledtrig-default-on_3.8.2-1_ar71xx.ipk
Size: 1596
MD5Sum: 891e004ce7a6d19e9e77da3fcc09a4bc
Description:  Kernel module that allows LEDs to be initialised in the ON state.

Package: kmod-ledtrig-heartbeat
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1652
Filename: kmod-ledtrig-heartbeat_3.8.2-1_ar71xx.ipk
Size: 2361
MD5Sum: 111f2a925138a506ab65ad3dafa469a2
Description:  LED Heartbeat Trigger

Package: kmod-ledtrig-netdev
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 3132
Filename: kmod-ledtrig-netdev_3.8.2-1_ar71xx.ipk
Size: 3823
MD5Sum: bea08b42a4c043415f30ee31681a53d6
Description:  Kernel module to drive LEDs based on network activity.

Package: kmod-ledtrig-timer
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1399
Filename: kmod-ledtrig-timer_3.8.2-1_ar71xx.ipk
Size: 2139
MD5Sum: 898bd9bc38f0e6eb369c780c75391928
Description:  Kernel module that allows LEDs to be controlled by a programmable timer
 via sysfs.

Package: kmod-ledtrig-usbdev
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-usb-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 2257
Filename: kmod-ledtrig-usbdev_3.8.2-1_ar71xx.ipk
Size: 2962
MD5Sum: fb6cab11031c12332b153118f36f29a0
Description:  Kernel module to drive LEDs based on USB device presence/activity.

Package: kmod-lib-crc-ccitt
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1374
Filename: kmod-lib-crc-ccitt_3.8.2-1_ar71xx.ipk
Size: 2075
MD5Sum: 98fcff4ac08633d5084ff2598f7dc6ab
Description:  Kernel module for CRC-CCITT support

Package: kmod-lib-textsearch
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 3546
Filename: kmod-lib-textsearch_3.8.2-1_ar71xx.ipk
Size: 4243
MD5Sum: 97ffe12ab6abd896056153ffacf1bae6
Description:  Textsearch support

Package: kmod-mac80211
Version: 3.8.2+2013-02-22-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-crypto-core, kmod-crypto-arc4, kmod-crypto-aes, kmod-cfg80211
Source: package/mac80211
SourceFile: compat-wireless-2013-02-22.tar.bz2
SourceURL: http://mirror2.openwrt.org/sources
Section: kernel
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 174137
Filename: kmod-mac80211_3.8.2+2013-02-22-1_ar71xx.ipk
Size: 173760
MD5Sum: 47b4ac0d8e9c00b4fcee5dc7c8386eb8
Description:  Generic IEEE 802.11 Networking Stack (mac80211)

Package: kmod-nls-base
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 3146
Filename: kmod-nls-base_3.8.2-1_ar71xx.ipk
Size: 3854
MD5Sum: 7cc82be962f91e22e05a51e3ee1ec888
Description:  Kernel module for NLS (Native Language Support)

Package: kmod-nls-cp1250
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-nls-base
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 2014
Filename: kmod-nls-cp1250_3.8.2-1_ar71xx.ipk
Size: 2721
MD5Sum: 84c56a980da5ccc0d5370d5fd2fa2fe9
Description:  Kernel module for NLS Codepage 1250 (Eastern Europe)

Package: kmod-nls-iso8859-15
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-nls-base
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1823
Filename: kmod-nls-iso8859-15_3.8.2-1_ar71xx.ipk
Size: 2521
MD5Sum: 03704f5b59f6ab700f5053b8385ddb01
Description:  Kernel module for NLS ISO 8859-15 (Latin 9)

Package: kmod-nls-iso8859-1
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-nls-base
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1715
Filename: kmod-nls-iso8859-1_3.8.2-1_ar71xx.ipk
Size: 2436
MD5Sum: 547f2111cc2325ae3ccc8bd48a1550c9
Description:  Kernel module for NLS ISO 8859-1 (Latin 1)

Package: kmod-nls-iso8859-2
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-nls-base
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1962
Filename: kmod-nls-iso8859-2_3.8.2-1_ar71xx.ipk
Size: 2656
MD5Sum: c69b8ebbca4d01d4c4513a1002c97e15
Description:  Kernel module for NLS ISO 8859-2 (Latin 2)

Package: kmod-nls-utf8
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-nls-base
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1024
Filename: kmod-nls-utf8_3.8.2-1_ar71xx.ipk
Size: 1724
MD5Sum: 608d588c9e43bcdcb267ef9b8b892fe0
Description:  Kernel module for NLS UTF-8

Package: kmod-ppp
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-lib-crc-ccitt
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 22518
Filename: kmod-ppp_3.8.2-1_ar71xx.ipk
Size: 23170
MD5Sum: f713534905ff00363e4a46b5c7e1fef6
Description:  Kernel modules for PPP support

Package: kmod-pppoe
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ppp, kmod-pppox
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 6157
Filename: kmod-pppoe_3.8.2-1_ar71xx.ipk
Size: 6864
MD5Sum: 9d07489a99e19ff261b947267eabae1c
Description:  Kernel module for PPPoE (PPP over Ethernet) support

Package: kmod-pppox
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ppp
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1696
Filename: kmod-pppox_3.8.2-1_ar71xx.ipk
Size: 2424
MD5Sum: f7596beb778d0127f499d040ccd995ab
Description:  Kernel helper module for PPPoE and PPTP support

Package: kmod-sched-connmark
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-sched-core, kmod-ipt-core, kmod-ipt-conntrack-extra
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 1275
Filename: kmod-sched-connmark_3.8.2-1_ar71xx.ipk
Size: 2013
MD5Sum: ecd41ad6b031a0ba17e78bdb29c5aed0
Description:  Traffic shaper conntrack mark support

Package: kmod-sched-core
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 34943
Filename: kmod-sched-core_3.8.2-1_ar71xx.ipk
Size: 35685
MD5Sum: 72443fdca6b9a7f20e6dbc31026f34b3
Description:  Core kernel scheduler support for IP traffic

Package: kmod-sit
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-ipv6, kmod-iptunnel4
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 9444
Filename: kmod-sit_3.8.2-1_ar71xx.ipk
Size: 10151
MD5Sum: 37c3a96f110b0883e958fdec33745fd4
Description:  Kernel modules for IPv6-in-IPv4 tunnelling

Package: kmod-usb-core
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-nls-base
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 69151
Filename: kmod-usb-core_3.8.2-1_ar71xx.ipk
Size: 69662
MD5Sum: 6db0150d663a4a41b5ad91f6c022badb
Description:  Kernel support for USB

Package: kmod-usb-ohci
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-usb-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 12422
Filename: kmod-usb-ohci_3.8.2-1_ar71xx.ipk
Size: 13091
MD5Sum: e2a2d8886fed9fa8334ac85f75a831d6
Description:  Kernel support for USB OHCI controllers

Package: kmod-usb-serial-option
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-usb-serial-wwan, kmod-usb-serial
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 8066
Filename: kmod-usb-serial-option_3.8.2-1_ar71xx.ipk
Size: 7924
MD5Sum: 284e47d4f6cccef3c81afaf5c7657a4d
Description:  Kernel support for Option HSDPA modems

Package: kmod-usb-serial-wwan
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-usb-serial
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 3753
Filename: kmod-usb-serial-wwan_3.8.2-1_ar71xx.ipk
Size: 4447
MD5Sum: be3e0c27c01913f0a71923729318b7dd
Description:  Kernel support for USB GSM and CDMA modems

Package: kmod-usb-serial
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-usb-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 12012
Filename: kmod-usb-serial_3.8.2-1_ar71xx.ipk
Size: 12702
MD5Sum: 0d5f7bf27ee5846d008bdf7c7cc8f6f5
Description:  Kernel support for USB-to-Serial converters

Package: kmod-usb2
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9), kmod-usb-core
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 22616
Filename: kmod-usb2_3.8.2-1_ar71xx.ipk
Size: 23275
MD5Sum: 1f6262f0f33d2e0ad235cba7b1f5a249
Description:  Kernel support for USB2 (EHCI) controllers

Package: kmod-wdt-ath79
Version: 3.8.2-1
Depends: kernel (=3.8.2-1-836a032e7c31b96a10e76637e90669d9)
Source: package/kernel
License: GPLv2
Section: kernel
Status: unknown hold not-installed
Architecture: ar71xx
Installed-Size: 3046
Filename: kmod-wdt-ath79_3.8.2-1_ar71xx.ipk
Size: 3736
MD5Sum: 34f9a17e91c5ef7cf126b7023864e10a
Description:  Kernel module for AR7XXX/AR9XXX watchdog timer.

Package: libblobmsg-json
Version: 2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442
Depends: libc, libjson, libubox
Source: package/libs/libubox
SourceFile: libubox-2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442.tar.gz
SourceURL: git://nbd.name/luci2/libubox.git
License: ISC BSD-3c
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 3334
Filename: libblobmsg-json_2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442_ar71xx.ipk
Size: 4006
MD5Sum: 64fc89c5d712a930d6e937510d98a451
Description:  blobmsg <-> json conversion library

Package: libdaemon
Version: 0.14-2
Depends: libc
Source: feeds/packages/libs/libdaemon
SourceFile: libdaemon-0.14.tar.gz
SourceURL: http://0pointer.de/lennart/projects/libdaemon/
Section: libs
Architecture: ar71xx
Installed-Size: 8042
Filename: libdaemon_0.14-2_ar71xx.ipk
Size: 8929
MD5Sum: d3d1120ed782cc868f98d1b5cc2f3ae5
Description:  libdaemon is a lightweight C library that eases the writing of UNIX daemons.
 It consists of the following parts:
 - A wrapper around fork() which does the correct daemonization procedure of a process
 - A wrapper around syslog() for simpler and compatible log output to Syslog or STDERR
 - An API for writing PID files
 - An API for serializing UNIX signals into a pipe for usage with select() or poll()
 - An API for running subprocesses with STDOUT and STDERR redirected to syslog
 
 APIs like these are used in most daemon software available. It is not that
 simple to get it done right and code duplication is not a goal.

Package: libgcc
Version: 4.6-linaro-1
Source: package/toolchain
Section: libs
Status: unknown hold not-installed
Essential: yes
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 31123
Filename: libgcc_4.6-linaro-1_ar71xx.ipk
Size: 31669
MD5Sum: 50ef587f94ce3aaba52e4f6dd0ed42c2
Description:  GCC support library

Package: libip4tc
Version: 1.4.18-2
Depends: libc
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: libs
Architecture: ar71xx
Installed-Size: 10032
Filename: libip4tc_1.4.18-2_ar71xx.ipk
Size: 10651
MD5Sum: d96d636a607c801615afdbe2b823795d
Description:  IPv4 firewall - shared libiptc library

Package: libip6tc
Version: 1.4.18-2
Depends: libc
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: libs
Architecture: ar71xx
Installed-Size: 10462
Filename: libip6tc_1.4.18-2_ar71xx.ipk
Size: 11093
MD5Sum: ba91aabe83f290b8b0dd4ae93995eccb
Description:  IPv6 firewall - shared libiptc library

Package: libiptc
Version: 1.4.18-2
Depends: libc, libip4tc, libip6tc
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: libs
Architecture: ar71xx
Installed-Size: 1019
Filename: libiptc_1.4.18-2_ar71xx.ipk
Size: 1664
MD5Sum: 5c1557052845ce055ace43a34a66f8bc
Description:  IPv4/IPv6 firewall - shared libiptc library (compatibility stub)

Package: libiwinfo-lua
Version: 39
Depends: libc, libiwinfo, liblua
Source: package/network/utils/iwinfo
Section: lang
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: ar71xx
Installed-Size: 6288
Filename: libiwinfo-lua_39_ar71xx.ipk
Size: 6787
MD5Sum: b5a25b69c1a77c701c011135e9454d4b
Description:  This is the Lua binding for the iwinfo library. It provides access to all enabled
 backends.

Package: libiwinfo
Version: 39
Depends: libc, libnl-tiny
Source: package/network/utils/iwinfo
Section: libs
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: ar71xx
Installed-Size: 21643
Filename: libiwinfo_39_ar71xx.ipk
Size: 22243
MD5Sum: 7989c1ae3c6e5864554d701085e27585
Description:  Wireless information library with consistent interface for proprietary Broadcom,
 madwifi, nl80211 and wext driver interfaces.

Package: libjson-script
Version: 2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442
Depends: libc, libubox
Source: package/libs/libubox
SourceFile: libubox-2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442.tar.gz
SourceURL: git://nbd.name/luci2/libubox.git
License: ISC BSD-3c
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 4968
Filename: libjson-script_2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442_ar71xx.ipk
Size: 5604
MD5Sum: 927098431decdd6d2435cb51498bf038
Description:  Minimalistic JSON based scripting engine

Package: libjson
Version: 0.9-2
Depends: libc
Source: package/libs/libjson-c
SourceFile: json-c-0.9.tar.gz
SourceURL: http://oss.metaparadigm.com/json-c/
License: MIT
LicenseFiles: COPYING
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 9439
Filename: libjson_0.9-2_ar71xx.ipk
Size: 10095
MD5Sum: 17bc00b304b353b72a99a35ed79bab5c
Description:  This package contains a library for javascript object notation backends.

Package: liblua
Version: 5.1.5-1
Depends: libc
Source: package/lua
SourceFile: lua-5.1.5.tar.gz
SourceURL: http://www.lua.org/ftp/ http://ftp.gwdg.de/pub/languages/lua/ http://mirrors.dotsrc.org/lua/ http://www.tecgraf.puc-rio.br/lua/ftp/
License: MIT
LicenseFiles: COPYRIGHT
Section: libs
Maintainer: Jo-Philipp Wich <jow@openwrt.org>
Architecture: ar71xx
Installed-Size: 72464
Filename: liblua_5.1.5-1_ar71xx.ipk
Size: 72755
MD5Sum: a5a6ec272834fbf2c498329188722ed1
Description:  Lua is a powerful light-weight programming language designed for extending 
 applications. Lua is also frequently used as a general-purpose, stand-alone 
 language. Lua is free software.
 This package contains the Lua shared libraries, needed by other programs.

Package: libnl-tiny
Version: 0.1-3
Depends: libc
Source: package/libs/libnl-tiny
License: GPLv2 LGPLv2.1
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 12718
Filename: libnl-tiny_0.1-3_ar71xx.ipk
Size: 13290
MD5Sum: bd9e17548d4e8fb3ba86e942a8d004a7
Description:  This package contains a stripped down version of libnl

Package: libpthread
Version: 0.9.33.2-1
Depends: libgcc
Source: package/toolchain
Section: libs
Status: unknown hold not-installed
Essential: yes
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 30757
Filename: libpthread_0.9.33.2-1_ar71xx.ipk
Size: 31345
MD5Sum: 55148b3ab6958041ba5bccb572afcefc
Description:  POSIX thread library

Package: librt
Version: 0.9.33.2-1
Depends: libpthread
Source: package/toolchain
Section: libs
Status: unknown hold not-installed
Essential: yes
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 4897
Filename: librt_0.9.33.2-1_ar71xx.ipk
Size: 5470
MD5Sum: 3af1d77955442da35d3fc6cc34d1a713
Description:  POSIX.1b RealTime extension library

Package: libubox
Version: 2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442
Depends: libc
Source: package/libs/libubox
SourceFile: libubox-2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442.tar.gz
SourceURL: git://nbd.name/luci2/libubox.git
License: ISC BSD-3c
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 11102
Filename: libubox_2013-03-05-49e6e062b8effe281a85de167c16c5f039b74442_ar71xx.ipk
Size: 11743
MD5Sum: 159c769b7325ac6269c2f179ad4a6d15
Description:  Basic utility library

Package: libubus-lua
Version: 2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0
Depends: libc, libubus, liblua
Source: package/ubus
SourceFile: ubus-2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0.tar.gz
SourceURL: git://nbd.name/luci2/ubus.git
License: LGPLv2.1
Section: luci2
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 4809
Filename: libubus-lua_2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0_ar71xx.ipk
Size: 5446
MD5Sum: 745f0a5417855e0b9ba195c954498d57
Description:  Lua binding for the OpenWrt RPC client

Package: libubus
Version: 2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0
Depends: libc, libubox
Source: package/ubus
SourceFile: ubus-2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0.tar.gz
SourceURL: git://nbd.name/luci2/ubus.git
License: LGPLv2.1
Section: luci2
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 11258
Filename: libubus_2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0_ar71xx.ipk
Size: 11901
MD5Sum: 35c7532430f3659cfe659b2ecf4e520f
Description:  OpenWrt RPC client library

Package: libuci-lua
Version: 2013-01-04.1-1
Depends: libc, libuci, liblua
Source: package/uci
SourceFile: uci-2013-01-04.1.tar.gz
SourceURL: git://nbd.name/uci.git
License: LGPLv2.1 GPLv2
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 6110
Filename: libuci-lua_2013-01-04.1-1_ar71xx.ipk
Size: 6717
MD5Sum: dc45561e5481c7dfdfd9fb3bb493c1a7
Description:  Lua plugin for UCI

Package: libuci
Version: 2013-01-04.1-1
Depends: libc
Source: package/uci
SourceFile: uci-2013-01-04.1.tar.gz
SourceURL: git://nbd.name/uci.git
License: LGPLv2.1 GPLv2
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 15235
Filename: libuci_2013-01-04.1-1_ar71xx.ipk
Size: 15843
MD5Sum: bc671020c2beba9f9ecc980c9da41d07
Description:  C library for the Unified Configuration Interface (UCI)

Package: libusb-1.0
Version: 1.0.9-1
Depends: libc, libpthread, librt
Source: package/libs/libusb
SourceFile: libusb-1.0.9.tar.bz2
SourceURL: @SF/libusb
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 22815
Filename: libusb-1.0_1.0.9-1_ar71xx.ipk
Size: 23428
MD5Sum: 08b04d042bd20d3115876b30f8d89a02
Description:  libusb is a C library that gives applications easy access to USB devices on
 many different operating systems.

Package: libusb-compat
Version: 0.1.4-1
Depends: libc, libusb-1.0
Source: package/libs/libusb-compat
SourceFile: libusb-compat-0.1.4.tar.bz2
SourceURL: @SF/libusb
Section: libs
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 5821
Filename: libusb-compat_0.1.4-1_ar71xx.ipk
Size: 6464
MD5Sum: 44fce36f874f235a05b2988e8a46cf96
Description:  libusb is a C library that gives applications easy access to USB devices on
 many different operating systems.

Package: libxtables
Version: 1.4.18-2
Depends: libc
Source: package/network/utils/iptables
SourceFile: iptables-1.4.18.tar.bz2
SourceURL: http://www.netfilter.org/projects/iptables/files ftp://ftp.be.netfilter.org/pub/netfilter/iptables/ ftp://ftp.de.netfilter.org/pub/netfilter/iptables/ ftp://ftp.no.netfilter.org/pub/netfilter/iptables/
Section: libs
Architecture: ar71xx
Installed-Size: 16745
Filename: libxtables_1.4.18-2_ar71xx.ipk
Size: 17323
MD5Sum: 432a373e6cb41924480588ce6ab62eaa
Description:  IPv4/IPv6 firewall - shared xtables library

Package: lua
Version: 5.1.5-1
Depends: libc, liblua
Source: package/lua
SourceFile: lua-5.1.5.tar.gz
SourceURL: http://www.lua.org/ftp/ http://ftp.gwdg.de/pub/languages/lua/ http://mirrors.dotsrc.org/lua/ http://www.tecgraf.puc-rio.br/lua/ftp/
License: MIT
LicenseFiles: COPYRIGHT
Section: lang
Maintainer: Jo-Philipp Wich <jow@openwrt.org>
Architecture: ar71xx
Installed-Size: 4702
Filename: lua_5.1.5-1_ar71xx.ipk
Size: 5454
MD5Sum: 0553dea8ffdeca6f10ed5f5c1ae05d04
Description:  Lua is a powerful light-weight programming language designed for extending 
 applications. Lua is also frequently used as a general-purpose, stand-alone 
 language. Lua is free software.
 This package contains the Lua language interpreter.

Package: luci-app-ddns
Version: trunk+svn9679-1
Depends: libc, ddns-scripts
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 11027
Filename: luci-app-ddns_trunk+svn9679-1_ar71xx.ipk
Size: 11633
MD5Sum: e6d89be5d1139ba433db9a31f58ebbaf
Description:  Dynamic DNS configuration module

Package: luci-app-firewall
Version: trunk+svn9679-1
Depends: libc, firewall3
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 52991
Filename: luci-app-firewall_trunk+svn9679-1_ar71xx.ipk
Size: 53682
MD5Sum: c7c5fd9faa30b13b74ba318e09085349
Description:  Firewall and Portforwarding application

Package: luci-app-qos
Version: trunk+svn9679-1
Depends: libc, qos-scripts
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 10017
Filename: luci-app-qos_trunk+svn9679-1_ar71xx.ipk
Size: 10682
MD5Sum: 4fca37da269bd646f4cfaf97a782a97c
Description:  Quality of Service configuration module

Package: luci-i18n-english
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 527
Filename: luci-i18n-english_trunk+svn9679-1_ar71xx.ipk
Size: 1240
MD5Sum: b5fc6cd9e1a5f9b35462f20a86a04365
Description:  English

Package: luci-i18n-french
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 21294
Filename: luci-i18n-french_trunk+svn9679-1_ar71xx.ipk
Size: 22063
MD5Sum: bf396f0b571c11ae75446d11e8d78664
Description:  French (by Florian Fainelli)

Package: luci-i18n-italian
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 9948
Filename: luci-i18n-italian_trunk+svn9679-1_ar71xx.ipk
Size: 10677
MD5Sum: 832eba4338ed6c175802b8f74ab60777
Description:  Italian (by Matteo Croce)

Package: luci-i18n-portuguese
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 7113
Filename: luci-i18n-portuguese_trunk+svn9679-1_ar71xx.ipk
Size: 7896
MD5Sum: f5b4ac4417d02e7edbeacde839d157f2
Description:  Portuguese (by Jose Monteiro)

Package: luci-i18n-romanian
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 8285
Filename: luci-i18n-romanian_trunk+svn9679-1_ar71xx.ipk
Size: 9044
MD5Sum: a71230129707910eebcc1f7d6e2b433c
Description:  Romanian

Package: luci-lib-core
Version: trunk+svn9679-1
Depends: libc, lua, libuci-lua, libubus-lua
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 30061
Filename: luci-lib-core_trunk+svn9679-1_ar71xx.ipk
Size: 30699
MD5Sum: 303855b146d6bed0f6a1ed7aa1d3510a
Description:  LuCI core libraries

Package: luci-lib-ipkg
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 2311
Filename: luci-lib-ipkg_trunk+svn9679-1_ar71xx.ipk
Size: 2915
MD5Sum: 24698381a61116188aefdd14e7bbbcdb
Description:  LuCI IPKG/OPKG call abstraction library

Package: luci-lib-nixio
Version: trunk+svn9679-1
Depends: libc, luci-lib-core
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 29410
Filename: luci-lib-nixio_trunk+svn9679-1_ar71xx.ipk
Size: 29793
MD5Sum: 38f6cf0d79c6ec910b5aeed5e80ab325
Description:  NIXIO POSIX library

Package: luci-lib-sys
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 16013
Filename: luci-lib-sys_trunk+svn9679-1_ar71xx.ipk
Size: 16615
MD5Sum: a61b23239d2e6bdfc8c0b65a23eaf8f5
Description:  LuCI Linux/POSIX system library

Package: luci-lib-web
Version: trunk+svn9679-1
Depends: libc, luci-lib-core, luci-lib-sys, luci-lib-nixio, luci-lib-core, luci-sgi-cgi
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 64873
Filename: luci-lib-web_trunk+svn9679-1_ar71xx.ipk
Size: 65618
MD5Sum: bf4b5f3fb91b9ffa8e8d8cb69491363a
Description:  MVC Webframework

Package: luci-mod-admin-core
Version: trunk+svn9679-1
Depends: libc, luci-lib-web, luci-proto-core, luci-i18n-english
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 5383
Filename: luci-mod-admin-core_trunk+svn9679-1_ar71xx.ipk
Size: 6134
MD5Sum: 1d5dbe9763cb2581e1d5469e57afa50e
Description:  Web UI Core module

Package: luci-mod-admin-full
Version: trunk+svn9679-1
Depends: libc, luci-mod-admin-core, luci-lib-ipkg
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 68765
Filename: luci-mod-admin-full_trunk+svn9679-1_ar71xx.ipk
Size: 69510
MD5Sum: 1371d45d55c45b7f17efabcb91b0dfd7
Description:  LuCI Administration - full-featured for full control

Package: luci-proto-3g
Version: trunk+svn9679-1
Depends: libc, comgt
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 1848
Filename: luci-proto-3g_trunk+svn9679-1_ar71xx.ipk
Size: 2436
MD5Sum: 63f5c3ed254afc0a69b7221fb88f792d
Description:  Support for 3G

Package: luci-proto-core
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 1894
Filename: luci-proto-core_trunk+svn9679-1_ar71xx.ipk
Size: 2511
MD5Sum: 78534140cde32044a8cadef5c48376bc
Description:  Support for static/dhcp/none

Package: luci-proto-ipv6
Version: trunk+svn9679-1
Depends: libc, 6in4, 6to4, 6rd, ipv6-support
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 2725
Filename: luci-proto-ipv6_trunk+svn9679-1_ar71xx.ipk
Size: 3347
MD5Sum: f62318c6b47369944a393782ede100b6
Description:  Support for DHCPv6/6in4/6to4/6rd

Package: luci-proto-ppp
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 3004
Filename: luci-proto-ppp_trunk+svn9679-1_ar71xx.ipk
Size: 3599
MD5Sum: ace19a414343c24644a6b1e24a57a46a
Description:  Support for PPP/PPPoE/PPPoA/PPtP

Package: luci-proto-relay
Version: trunk+svn9679-1
Depends: libc, relayd
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 2210
Filename: luci-proto-relay_trunk+svn9679-1_ar71xx.ipk
Size: 2839
MD5Sum: d4014559ffe573bad80f87c8493a2f3c
Description:  Support for relayd pseudo bridges

Package: luci-sgi-cgi
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 1491
Filename: luci-sgi-cgi_trunk+svn9679-1_ar71xx.ipk
Size: 2129
MD5Sum: dd1199d7d7e3cfb6b60b7420aeafa2c0
Description:  CGI Gateway behind existing Webserver

Package: luci-theme-base
Version: trunk+svn9679-1
Depends: libc
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 23542
Filename: luci-theme-base_trunk+svn9679-1_ar71xx.ipk
Size: 24140
MD5Sum: e85f93e2330ae33dd1c7af8d13240fb9
Description:  Common base for all themes

Package: luci-theme-bootstrap
Version: trunk+svn9679-1
Depends: libc, luci-theme-base
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 12791
Filename: luci-theme-bootstrap_trunk+svn9679-1_ar71xx.ipk
Size: 13499
MD5Sum: 8f849564de4142e87eed077861c4e1c2
Description:  Bootstrap Theme

Package: luci-theme-freifunk-generic
Version: trunk+svn9679-1
Depends: libc, luci-theme-base
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: Manuel Munz <freifunk-at-somakoma-dot-de>
Architecture: ar71xx
Installed-Size: 12970
Filename: luci-theme-freifunk-generic_trunk+svn9679-1_ar71xx.ipk
Size: 13719
MD5Sum: c1a5836711ca9c12b8ef51952f01fb3d
Description:  Freifunk Generic Theme

Package: luci-theme-openwrt
Version: trunk+svn9679-1
Depends: libc, luci-theme-base
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 7090
Filename: luci-theme-openwrt_trunk+svn9679-1_ar71xx.ipk
Size: 7868
MD5Sum: f36b010aeb5ef1370ab93bdae2c96f95
Description:  OpenWrt.org (default)

Package: luci
Version: trunk+svn9679-1
Depends: libc, uhttpd, uhttpd-mod-ubus, luci-mod-admin-full, luci-theme-openwrt, luci-app-firewall, luci-proto-core, luci-proto-ppp, libiwinfo-lua
Source: feeds/luci/luci
SourceFile: luci-trunk+svn9679.tar.gz
SourceURL: http://svn.luci.subsignal.org/luci/trunk
Section: luci
Maintainer: LuCI Development Team <luci@lists.subsignal.org>
Architecture: ar71xx
Installed-Size: 106
Filename: luci_trunk+svn9679-1_ar71xx.ipk
Size: 802
MD5Sum: 27d2364b16364273e73aec25942ac4ab
Description:  Standard OpenWrt set including full admin with ppp support and the default OpenWrt theme

Package: mtd
Version: 20
Depends: libc
Source: package/mtd
License: GPLv2 GPLv2+
Section: utils
Architecture: ar71xx
Installed-Size: 10528
Filename: mtd_20_ar71xx.ipk
Size: 11093
MD5Sum: c6cff862e74d78a4e61a1e6e301c07c6
Description:  This package contains an utility useful to upgrade from other firmware or 
 older OpenWrt releases.

Package: netifd
Version: 2013-02-19-486aa750a164d41905beb61afec89268e3eb7f48
Depends: libc, libuci, libnl-tiny, libubus, ubus, ubusd, jshn
Source: package/network/config/netifd
SourceFile: netifd-2013-02-19-486aa750a164d41905beb61afec89268e3eb7f48.tar.gz
SourceURL: git://nbd.name/luci2/netifd.git
License: GPLv2
Section: base
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 41041
Filename: netifd_2013-02-19-486aa750a164d41905beb61afec89268e3eb7f48_ar71xx.ipk
Size: 41312
MD5Sum: a9f91e13adc9acf2a017f431f5305bab
Description:  OpenWrt Network Interface Configuration Daemon

Package: odhcp6c
Version: 2013-03-08-e8b07f018cbdf8f2a08f93af46904e7ffb9eb123
Depends: libc, kmod-ipv6
Source: package/network/ipv6/odhcp6c
SourceFile: odhcp6c-2013-03-08.tar.bz2
SourceURL: git://github.com/sbyx/odhcp6c.git
Section: ipv6
Maintainer: Steven Barth <steven@midlink.org>
Architecture: ar71xx
Installed-Size: 13886
Filename: odhcp6c_2013-03-08-e8b07f018cbdf8f2a08f93af46904e7ffb9eb123_ar71xx.ipk
Size: 14503
MD5Sum: 5765784ec84e5218ba993074051f16f1
Description:  Embedded DHCPv6-client for OpenWrt

Package: opkg
Version: 618-3
Depends: libc
Source: package/opkg
SourceFile: opkg-618.tar.gz
SourceURL: http://opkg.googlecode.com/svn/trunk/
License: GPLv2
LicenseFiles: COPYING
Section: base
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: ar71xx
Installed-Size: 56693
Filename: opkg_618-3_ar71xx.ipk
Size: 57166
MD5Sum: f676afb04cef3d58d47079b163fe0dd6
Description:  Lightweight package management system
 opkg is the opkg Package Management System, for handling
 installation and removal of packages on a system. It can
 recursively follow dependencies and download all packages
 necessary to install a particular package.
 
 opkg knows how to install both .ipk and .deb packages.

Package: ppp-mod-pppoe
Version: 2.4.5-9
Depends: libc, kmod-pppoe
Source: package/network/services/ppp
SourceFile: ppp-2.4.5.tar.gz
SourceURL: ftp://ftp.samba.org/pub/ppp/
Section: net
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: ar71xx
Installed-Size: 8442
Filename: ppp-mod-pppoe_2.4.5-9_ar71xx.ipk
Size: 9089
MD5Sum: 216dbb9f2ebeb0b058b0973797536ab5
Description:  This package contains a PPPoE (PPP over Ethernet) plugin for ppp.

Package: ppp
Version: 2.4.5-9
Depends: libc, kmod-ppp
Source: package/network/services/ppp
SourceFile: ppp-2.4.5.tar.gz
SourceURL: ftp://ftp.samba.org/pub/ppp/
Section: net
Maintainer: Jo-Philipp Wich <xm@subsignal.org>
Architecture: ar71xx
Installed-Size: 103477
Filename: ppp_2.4.5-9_ar71xx.ipk
Size: 103699
MD5Sum: c76483e4bedfbb2b9d70134c9b611e6e
Description:  This package contains the PPP (Point-to-Point Protocol) daemon.

Package: procd
Version: 2013-03-13-8158e9052afbf2ee47de645167b90b6e7fc7d86d
Depends: libc, ubusd, ubus, libjson-script
Source: package/procd
SourceFile: procd-2013-03-13-8158e9052afbf2ee47de645167b90b6e7fc7d86d.tar.gz
SourceURL: git://nbd.name/luci2/procd.git
License: GPLv2
Section: base
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 20409
Filename: procd_2013-03-13-8158e9052afbf2ee47de645167b90b6e7fc7d86d_ar71xx.ipk
Size: 20744
MD5Sum: 5121f7d0afb7b73c27e44efcbe5ee43f
Description:  OpenWrt system process manager

Package: qos-scripts
Version: 1.2.1-6
Depends: libc, tc, kmod-sched-core, kmod-sched-connmark, kmod-ifb, iptables, iptables-mod-filter, iptables-mod-ipopt, iptables-mod-conntrack-extra
Source: package/network/config/qos-scripts
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: all
Installed-Size: 6144
Filename: qos-scripts_1.2.1-6_all.ipk
Size: 6824
MD5Sum: 9f907907c5752df8f1cc53926a36b21c
Description:  A set of scripts that abstract QoS configuration into a simple 
 configuration file supporting stanzas that specify any number of QoS 
 entries.

Package: relayd
Version: 2011-10-24-4e8f1fa4ca2b176500362843a9e57ea5abd4b7a3
Depends: libc, libubox
Source: package/network/services/relayd
SourceFile: relayd-2011-10-24.tar.bz2
SourceURL: git://nbd.name/relayd.git
Section: net
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 9547
Filename: relayd_2011-10-24-4e8f1fa4ca2b176500362843a9e57ea5abd4b7a3_ar71xx.ipk
Size: 10184
MD5Sum: 4bb2e032b1e779d083c4a28350df4090
Description:  Transparent routing / relay daemon

Package: restorefactory
Version: 1-6
Depends: libc
Source: feeds/packages/utils/restorefactory
Section: utils
Maintainer: Nuno Goncalves <nunojpg@gmail.com>
Architecture: ar71xx
Installed-Size: 664
Filename: restorefactory_1-6_ar71xx.ipk
Size: 1296
MD5Sum: 7c6344ffdff2a5db61225586ca0ed0f5
Description:  RestoreFactory handles the reset button event and issues a "firstboot" command.
 Button and wait time can be configured with a UCI file.

Package: swconfig
Version: 10
Depends: libc, libuci, libnl-tiny
Source: package/network/config/swconfig
Section: base
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 7041
Filename: swconfig_10_ar71xx.ipk
Size: 7626
MD5Sum: f2e52a6c862470a031209a7662d4ccfb
Description:  Switch configuration utility

Package: tc
Version: 3.7.0-1
Depends: libc, kmod-sched-core
Source: package/network/utils/iproute2
SourceFile: iproute2-3.7.0.tar.bz2
SourceURL: http://kernel.org/pub/linux/utils/net/iproute2/
Section: net
Architecture: ar71xx
Installed-Size: 95530
Filename: tc_3.7.0-1_ar71xx.ipk
Size: 96045
MD5Sum: aee1335f8f1a4893019747d596f4ed61
Description:  Traffic control utility

Package: uboot-envtools
Version: 2012.04.01-1
Depends: libc
Source: package/boot/uboot-envtools
SourceFile: u-boot-2012.04.01.tar.bz2
SourceURL: ftp://ftp.denx.de/pub/u-boot
Section: utils
Architecture: ar71xx
Installed-Size: 9234
Filename: uboot-envtools_2012.04.01-1_ar71xx.ipk
Size: 9830
MD5Sum: f513a04d05c15bbc2d7a6b7f95afab57
Description:  This package includes tools to read and modify U-Boot bootloader environment.

Package: ubus
Version: 2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0
Depends: libc, libubus, libblobmsg-json, ubusd
Source: package/ubus
SourceFile: ubus-2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0.tar.gz
SourceURL: git://nbd.name/luci2/ubus.git
License: LGPLv2.1
Section: luci2
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 3399
Filename: ubus_2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0_ar71xx.ipk
Size: 4071
MD5Sum: 050f8a9770968cbe8a0624588fdd5d8a
Description:  OpenWrt RPC client utility

Package: ubusd
Version: 2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0
Depends: libc, libubox
Source: package/ubus
SourceFile: ubus-2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0.tar.gz
SourceURL: git://nbd.name/luci2/ubus.git
License: LGPLv2.1
Section: luci2
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 7144
Filename: ubusd_2013-03-06-495f4608189049495c7b4f6c5198bba556d6e9b0_ar71xx.ipk
Size: 7823
MD5Sum: 229f047149467785d0a7033e07f4afdf
Description:  OpenWrt RPC daemon

Package: uci
Version: 2013-01-04.1-1
Depends: libc, libuci
Source: package/uci
SourceFile: uci-2013-01-04.1.tar.gz
SourceURL: git://nbd.name/uci.git
License: LGPLv2.1 GPLv2
Section: base
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 6804
Filename: uci_2013-01-04.1-1_ar71xx.ipk
Size: 7490
MD5Sum: 2ed5ce4f64fcef9232f12c2be70ebc8e
Description:  Utility for the Unified Configuration Interface (UCI)

Package: uhttpd-mod-ubus
Version: 2013-01-22-14e3971c37e6feb0ec5eda0988e07d8a786ba9f9
Depends: libc, uhttpd, libubus, libblobmsg-json
Source: package/network/services/uhttpd
SourceFile: uhttpd-2013-01-22-14e3971c37e6feb0ec5eda0988e07d8a786ba9f9.tar.gz
SourceURL: git://nbd.name/uhttpd2.git
Section: net
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 7931
Filename: uhttpd-mod-ubus_2013-01-22-14e3971c37e6feb0ec5eda0988e07d8a786ba9f9_ar71xx.ipk
Size: 8681
MD5Sum: 9c9de7d778376c526f611550c3609a1d
Description:  The ubus plugin adds a HTTP/JSON RPC proxy for ubus and publishes the
 session.* namespace and procedures.

Package: uhttpd
Version: 2013-01-22-14e3971c37e6feb0ec5eda0988e07d8a786ba9f9
Depends: libc, libubox
Source: package/network/services/uhttpd
SourceFile: uhttpd-2013-01-22-14e3971c37e6feb0ec5eda0988e07d8a786ba9f9.tar.gz
SourceURL: git://nbd.name/uhttpd2.git
Section: net
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 20035
Filename: uhttpd_2013-01-22-14e3971c37e6feb0ec5eda0988e07d8a786ba9f9_ar71xx.ipk
Size: 20662
MD5Sum: 143805084da30c6bb810f4532f68cff9
Description:  uHTTPd is a tiny single threaded HTTP server with TLS, CGI and Lua
 support. It is intended as a drop-in replacement for the Busybox
 HTTP daemon.

Package: usb-modeswitch-data
Version: 20121109
Depends: libc, usb-modeswitch
Source: package/system/utils/usb-modeswitch
SourceFile: usb-modeswitch-1.2.5.tar.bz2
SourceURL: http://www.draisberghof.de/usb_modeswitch
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 13378
Filename: usb-modeswitch-data_20121109_ar71xx.ipk
Size: 13598
MD5Sum: 95d05d726ad3d65994773f22205fda2d
Description:  Configuration database for usb-modeswitch.
 Contains definitions for many USB devices required to
 autoswitch "flip flop" gear.

Package: usb-modeswitch
Version: 1.2.5-1
Depends: libc, libusb-compat
Source: package/system/utils/usb-modeswitch
SourceFile: usb-modeswitch-1.2.5.tar.bz2
SourceURL: http://www.draisberghof.de/usb_modeswitch
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 17345
Filename: usb-modeswitch_1.2.5-1_ar71xx.ipk
Size: 18040
MD5Sum: 8515fb9fb559ab6e11386e6f9d664562
Description:  A mode switching tool for controlling
 "flip flop" (multiple device) USB gear.

Package: usbutils
Version: 006-1
Depends: libc, libusb-1.0, zlib, librt, libpthread
Source: package/system/utils/usbutils
SourceFile: usbutils-006.tar.bz2
SourceURL: @KERNEL/linux/utils/usb/usbutils
Section: utils
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 196339
Filename: usbutils_006-1_ar71xx.ipk
Size: 197107
MD5Sum: 7193a5a1c6e7d1e5cd6fc82bfb7b00cb
Description:  USB devices listing utilities

Package: wifitoggle
Version: 1-3
Depends: libc
Source: feeds/packages/utils/wifitoggle
Section: utils
Maintainer: Nuno Goncalves <nunojpg@gmail.com>
Architecture: ar71xx
Installed-Size: 1487
Filename: wifitoggle_1-3_ar71xx.ipk
Size: 2181
MD5Sum: 3349e20104199a2f6f6ce9045b97ab91
Description:  Very versatile script to toggle Wi-Fi with a button. Allows to set
 timeouts, persist changes after boot, and set LEDs according to the state.

Package: wpad-mini
Version: 20130302-1
Depends: libc, libnl-tiny
Source: package/network/services/hostapd
SourceFile: hostapd-20130302.tar.bz2
SourceURL: git://w1.fi/srv/git/hostap.git
Section: net
Maintainer: Felix Fietkau <nbd@openwrt.org>
Architecture: ar71xx
Installed-Size: 183740
Filename: wpad-mini_20130302-1_ar71xx.ipk
Size: 184003
MD5Sum: bcea6a093adfe1a71df95f8c9de1b602
Description:  This package contains a minimal IEEE 802.1x/WPA Authenticator and Supplicant (WPA-PSK only).

Package: zlib
Version: 1.2.7-1
Depends: libc
Source: package/libs/zlib
SourceFile: zlib-1.2.7.tar.bz2
SourceURL: http://www.zlib.net @SF/libpng
License: ZLIB
LicenseFiles: README
Section: libs
Architecture: ar71xx
Installed-Size: 39601
Filename: zlib_1.2.7-1_ar71xx.ipk
Size: 40232
MD5Sum: 27c3582d18fc109b96084a3ebe3a7df8
Description:  Library implementing the deflate compression method

